**STARTING, STOPPING, AND STORAGE**

**(Do not use collapsible Garden Hose)**

**To Start:**

1. **Un-coil ¾” Garden Hose, turn on water and flush out** (this cleans the inside of the hose, and removes most of the air)
2. **Connect Garden and High-Pressure Hoses to Pressure Washer, connect Gun, turn Garden Hose water flow “ON”, squeeze trigger on Gun and hold open for 3 MINUTES** (this purges the air from both the hoses and the PUMP)**.**
3. **Turn on Gas Lever (when applicable), switch choke to FULL/ON position, and turn Ignition to “ON” position.**
4. **Lastly, insert COLORED NOZZLE into end of gun (when applicable), squeeze trigger on Gun, and pull start the engine.**
5. **After engine starts, move choke lever to ½ way position, and run engine for 15 seconds on ½ choke; then, move choke to “OFF” position, and start pressure washing.**

**To Stop/Store:**

1. **Turn Gas Lever (when applicable) to “OFF” position, continue to spray water through the Gun until the engine stops; it should take about 60 seconds. Release all pressure through the Gun, disconnect all Hoses, and disconnect Gun.**
2. **Lastly, fill Gas Tank with treated fuel and store away! (NOTE: ONLY USE FUEL THAT HAS PREVIOUSLY BEEN TREATED, IN THE GAS CAN, WITH ETHANOL TREATMENT)**
3. **If your pump is a “Store Brand” (i.e. Briggs and Stratton, Stihl, TroyBilt, Craftsman, Karcher, etc..) Also, use a PUMP STORAGE PRODUCT.**